|  |
| --- |
| Refrigerant Identifiers  |
| Part No  | **Description** | **HFO1234yf** | **R134, R12, R22, HC & AIR** |
| 41-0062A | Mini Refrigerant Identifier  |
| * Easy to use with ‘PASS’ or ‘FAIL’ LED indication
* ‘FAULT’ and ‘EXCESS AIR’ LEDs
* Step by step LED indications of the gas sampling process
* Compact and lightweight design
* Rugged construction and housing
* Hand-held and extremely portable
 | **The new, low cost Mini ID Refrigerant Identifier helps verify the presence and quality of HFO1234yf refrigerant in vehicle** **air conditioning systems thus preventing possible contamination and damage to service and recovery equipment.**  |
| **The Mini ID delivers** **fast and accurate****refrigerant** **analysing. It is self** **contained, compact** **and comes in an** **extremely portable and rugged ABS case and is very simple** **to use.**   |  |
|  Technical Specifications* Weight:

8.0 lb* Power requirements:

12-15VDC, Optional battery pack (Internal)* Output:

Digital display and LEDs * Refrigerant:

HFO1234yf,R12, R134a, R22, HC and Air* Display:

128 x 64 Pixel Graphing* Resolution:

0.1%* Operating humidity:

0-95% RH non-condensing* Operating temperature:

40°F to 130°F* Warranty:

1 yr.* Approvals:

SAE J1771, CE, UL | Easy to use ‘PASS’ or 'FAIL' result indicationCompact andlightweight design   'FAULT' &'EXCESS AIR' indicationRugged and tough designSimple gas Indicationwhile SamplingHand-Held and extremely portable     |